**Main Reserve Switch**

The Main/Reserve Switch shall be capable of switching the release output of a release panel to either a primary (main) or secondary (reserve) source of extinguishing agent.

The unit shall consist of a UL, CUL Listed DPDT key operated switch rated for 1 Amp at 40 VDC mounted to a stainless steel faceplate with a green and yellow LED. The green LED shall be labeled Main and shall only light when the key is in the main position. The yellow LED shall be labeled Reserve and shall only light when the switch is in the reserve position. The Key shall be removable in either position. The unit shall be designed to mount on a standard single gang enclosure.

The Main / Reserve Switch shall be a Potter model MRS or equivalent.