**Sprinkler Alarm Horn Strobe and Sign Combination**

cULus Listed. The contractor shall furnish and install a Strobe Horn / sign combination.

The device shall consist of a weatherproof strobe horn of the applicable voltage, weatherproof backbox and red non corrosive sign with white lettering identifying it as a sprinkler alarm with instructions to contact the fire department or 911.

Sprinkler Alarm Strobe Horn shall be a Potter Electric Signal model SASH12/24 for 12 or 24VDC operation or SASH120 for 120 VAC operation. SASH 120 is UL Listed only.